Specifications

* Frameset

**Frame**

OCLV Mountain Carbon main frame, alloy stays, ABP, Boost148, Knock Block steerer stop, Full Floater, EVO link, tapered head tube, Mino Link, Control Freak internal routing, Carbon Armor, PF92, ISCG 05, G2 Geometry, 130mm travel

**Fork**

Fox Rhythm 34 Float, GRIP adjustable damper, tapered steerer, G2 Geometry w/51mm offset, Boost110, 130mm travel

**Rear suspension**

Fox Performance Float EVOL, RE:aktiv 3-position damper, tuned by Trek Suspension Lab, 210x52.5mm

* Wheels

**Wheels**

Bontrager Line Comp 30, Tubeless Ready, 54T Rapid Drive, Boost110 front, Boost148 rear, tubeless strips included, valves sold separately

**Tires**

Bontrager XR4 Team Issue, Tubeless Ready, Inner Strength sidewalls, 120tpi, aramid bead, 29x2.40˝

* Drivetrain

**Shifters**

SRAM NX Eagle, 12 speed

**Rear derailleur**

SRAM GX Eagle, Roller Bearing Clutch

**Crank**

Truvativ Descendant 6k Eagle DUB, 32T Direct Mount

**Bottom bracket**

SRAM DUB Press Fit, 92mm

**Cassette**

SRAM XG-1230 Eagle, 11-50, 12 speed

**Chain**

SRAM NX Eagle

**Pedals**

Not included

* Components

**Saddle**

Bontrager Arvada, hollow chromoly rails

**Seatpost**

Bontrager Line, internal routing, 31.6mm, 15.5: 100mm, 17.5 & 18.5: 125mm, 19.5 & 21.5: 150mm

**Handlebar**

Bontrager Line, 35mm, 15mm rise, 750mm width

**Grips**

Bontrager XR Trail Elite, alloy lock-on

**Stem**

Bontrager Line, Knock Block, 35mm clamp, 0 degree

**Headset**

Knock Block Integrated, sealed cartridge bearing, 1-1/8˝ top, 1.5˝ bottom

**Brakeset**

Shimano Deore M6000 hydraulic disc

* Weight

**Weight**

M - 13.65 kg / 30.1 lbs (with tubes)

**Weight limit**

This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 300 pounds (136 kg).