Specifications

* Frameset

**Frame**

500 Series OCLV Carbon, Front & Rear IsoSpeed, tapered head tube, BB90, flat mount disc brakes, 12mm thru-axle, internal cable routing, hidden fender mounts, 3S chain keeper, DuoTrap S compatible, Ride Tuned seatmast

**Fork**

Domane carbon disc, carbon tapered steerer, flat mount disc brakes, 12mm thru-axle

* Wheels

**Wheels**

Bontrager Paradigm Disc Tubeless Ready, 12mm thru-axle

**Tires**

Bontrager R2 Hard-Case Lite, aramid bead, 700x32c

**Max tire size**

32c Bontrager tires (with at least 4mm of clearance to frame)

* Drivetrain

**Shifters**

Shimano Ultegra, 11 speed

**Front derailleur**

Shimano Ultegra, braze-on

**Rear derailleur**

Shimano Ultegra, 11 speed

**Crank**

Shimano Ultegra, 50/34 (compact)

**Bottom bracket**

BB90

**Cassette**

Shimano Ultegra, 11-34, 11 speed

**Chain**

Shimano Ultegra

**Pedals**

Not included

* Components

**Saddle**

Bontrager Ajna Comp, chromoly rails

**Seatpost**

Bontrager Ride Tuned carbon seatmast cap, 20mm offset

**Handlebar**

Bontrager Elite IsoZone VR-SF, 31.8mm

**Grips**

Bontrager tape

**Stem**

Bontrager Pro, 31.8mm, 7 degree, w/computer & light mounts

**Headset**

Integrated, cartridge bearing, sealed, 1-1/8˝ top, 1.5˝ bottom

**Brakeset**

Shimano Ultegra flat mount hydraulic disc

* Weight

**Weight**

54cm - 8.51 kg / 18.77 lbs

**Weight limit**

This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 275 pounds (125 kg).