Specifications

* Frameset

**Frame**

Ultralight 300 Series Alpha Aluminum, Invisible Weld Technology, tapered head tube, BB86.5, flat mount disc brakes, 12mm thru-axle, internal cable routing, DuoTrap S compatible

**Fork**

Émonda carbon disc, carbon tapered steerer, flat mount disc brakes, 12mm thru-axle

* Wheels

**Front hub**

Bontrager alloy sealed bearing, 12mm thru-axle

**Rear hub**

Bontrager alloy sealed bearing, 12mm thru-axle

**Rims**

Bontrager Affinity Tubeless Ready Disc

**Tires**

Bontrager R1 Hard-Case Lite, 700x 25c

**Max tire size**

28c Bontrager tires (with at least 4mm of clearance to frame)

* Drivetrain

**Shifters**

Shimano 105, 11 speed

**Front derailleur**

Shimano 105, braze-on

**Rear derailleur**

Shimano 105

**Crank**

Shimano 105, 50/34 (compact)

**Bottom bracket**

Press Fit BB86.5

**Cassette**

Shimano 105, 11-28, 11 speed

**Chain**

Shimano 105

**Pedals**

Not included

* Components

**Saddle**

Bontrager Montrose Comp, chromoly rails

**Seatpost**

Bontrager carbon, 2-bolt head, 27.2mm, 8mm offset

**Handlebar**

Bontrager Comp VR-C, 31.8mm

**Grips**

Bontrager tape

**Stem**

Bontrager Elite, 31.8mm, 7 degree, w/computer & light mounts

**Headset**

Integrated, cartridge bearing, sealed, 1-1/8˝ top, 1.5˝ bottom

**Brakeset**

Shimano 105 flat mount hydraulic disc

* Weight

**Weight**

8.98 kg / 19.79 lbs

**Weight limit**

This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 275 pounds (125 kg).