Specifications

* Frameset

**Frame**

700 Series OCLV Carbon, KVF (Kammtail Virtual Foil) tube shape, Adjustable Top Tube IsoSpeed, Micro-adjust seatmast, tapered head tube, BB90, direct mount rim brakes, invisible cable routing, control center, precision water bottle placement, Aero 3S chain keeper, DuoTrap S compatible

**Fork**

Madone KVF full carbon, carbon tapered steerer, carbon dropouts, Madone integrated brake

* Wheels

**Wheels**

Bontrager Aeolus Pro 5 Tubeless Ready

**Tires**

Bontrager R3 Hard-Case Lite, 120 tpi, aramid bead, 700x25c

**Max tire size**

25c Bontrager tires (with at least 4mm of clearance to frame)

* Drivetrain

**Shifters**

Shimano Dura-Ace, 11 speed

**Front derailleur**

Shimano Dura-Ace, braze-on

**Rear derailleur**

Shimano Dura-Ace

**Crank**

Shimano Dura-Ace, 50/34 (compact)

**Bottom bracket**

BB90

**Cassette**

Shimano Dura-Ace, 11-28, 11 speed

**Chain**

Shimano Dura-Ace

**Pedals**

Not included

* Components

**Saddle**

Bontrager Montrose Elite, titanium rails

**Seatpost**

Madone carbon seatpost, 25mm offset w/integrated light mount

**Handlebar**

Madone specific adjustable aero VR-CF, internal cable routing

**Grips**

Bontrager tape

**Stem**

Madone specific internal cable routing

**Headset**

Madone integrated, stainless cartridge bearings, sealed, 1-3/8˝ top, 1.5˝ bottom

**Brakeset**

Madone aero, integrated

* Weight

**Weight**

56cm - 7.35 kg / 16.2 lbs

**Weight limit**

This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 275 pounds (125 kg).