Specifications

*\*spec applies to all sizes unless otherwise noted*

[**Frameset**](https://www.trekbikes.com/us/en_US/bikes/road-bikes/performance-road-bikes/domane/domane-sl/domane-sl-6/p/28313/?colorCode=black)

|  |  |
| --- | --- |
| Frame | 500 Series OCLV Carbon, front & rear IsoSpeed, internal storage, tapered head tube, internal cable routing, micro-adjust seat mast, 3S chain keeper, DuoTrap S compatible, fender mounts, flat mount disc, 142x12mm thru axle |
| \*Fork | Size: 44, 47 Domane SLR carbon, tapered carbon steerer, internal brake routing, fender mounts, flat mount disc, carbon dropouts, 12x100mm thru axle |
| Size: 50, 52, 54, 56, 58, 60, 62 Domane SL carbon, tapered carbon steerer, internal brake routing, fender mounts, flat mount disc, 12x100mm thru axle |

[**Wheels**](https://www.trekbikes.com/us/en_US/bikes/road-bikes/performance-road-bikes/domane/domane-sl/domane-sl-6/p/28313/?colorCode=black)

|  |  |
| --- | --- |
| Front Wheel | Bontrager Paradigm Comp 25, Tubeless Ready, 25mm rim width, 100x12mm thru axle |
| Rear Wheel | Bontrager Paradigm Comp 25, Tubeless Ready, 25mm rim width, Shimano 11-speed freehub, 142x12 thru axle |
| Tire | Bontrager R2 Hard-Case Lite, aramid bead, 60 tpi, 700x32c |

[**Drivetrain**](https://www.trekbikes.com/us/en_US/bikes/road-bikes/performance-road-bikes/domane/domane-sl/domane-sl-6/p/28313/?colorCode=black)

|  |  |
| --- | --- |
| \*Shifter | Size: 44, 47, 50, 52 Shimano Ultegra R8025, short-reach lever, 11 speed |
| Size: 54, 56, 58, 60, 62 Shimano Ultegra R8020, 11-speed |
| Front Derailleur | Shimano Ultegra R8000, braze-on |
| Rear Derailleur | Shimano Ultegra R8000, long cage, 34T max cog |
| \*Crank | Size: 44, 47 Shimano Ultegra R8000, 50/34 (compact), 165mm length |
| Size: 50, 52 Shimano Ultegra R8000, 50/34 (compact), 170mm length |
| Size: 54, 56 Shimano Ultegra R8000, 50/34 (compact), 172.5mm length |
| Size: 58, 60, 62 Shimano Ultegra R8000, 50/34 (compact), 175mm length |
| Bottom Bracket | Praxis, T47 threaded, internal bearing |
| Cassette | Shimano Ultegra HG800-11, 11-34, 11 speed |
| Chain | Shimano Ultegra HG701, 11-speed |

[**Components**](https://www.trekbikes.com/us/en_US/bikes/road-bikes/performance-road-bikes/domane/domane-sl/domane-sl-6/p/28313/?colorCode=black)

|  |  |
| --- | --- |
| Saddle | [Bontrager Arvada Comp, steel rails, 154mm width](https://www.trekbikes.com/p/549169) |
| \*Seatpost | Size: 44, 47, 50, 52, 54, 56 Bontrager carbon seatmast cap, integrated light mount, 20mm offset, 135mm length (short) |
| Size: 58, 60, 62 Bontrager carbon seatmast cap, integrated light mount, 20mm offset, 175mm length (long) |
| \*Handlebar | Size: 44, 47 Bontrager Elite IsoZone VR-SF, alloy, 31.8mm, internal Di2 routing, 75mm reach, 128mm drop, 36cm width |
| Size: 50 Bontrager Elite IsoZone VR-SF, alloy, 31.8mm, internal Di2 routing, 75mm reach, 128mm drop, 38cm width |
| Size: 52 Bontrager Elite IsoZone VR-SF, alloy, 31.8mm, internal Di2 routing, 75mm reach, 128mm drop, 40cm width |
| Size: 54, 56 Bontrager Elite IsoZone VR-CF, alloy, 31.8mm, internal Di2 routing, 93mm reach, 123mm drop, 42cm width |
| Size: 58, 60, 62 Bontrager Elite IsoZone VR-CF, alloy, 31.8mm, internal Di2 routing, 93mm reach, 123mm drop, 44cm width |
| Handlebar Tape | [Bontrager Supertack Perf tape](https://www.trekbikes.com/p/503320) |
| \*Stem | Size: 44 Bontrager Pro, 31.8mm, Blendr compatible, 7 degree, 60mm length |
| Size: 47 Bontrager Pro, 31.8mm, Blendr compatible, 7 degree, 70mm length |
| Size: 50 [Bontrager Pro, 31.8mm, Blendr compatible, 7 degree, 80mm length](https://www.trekbikes.com/p/564743) |
| Size: 52, 54 [Bontrager Pro, 31.8mm, Blendr compatible, 7 degree, 90mm length](https://www.trekbikes.com/p/564744) |
| Size: 56, 58 [Bontrager Pro, 31.8mm, Blendr compatible, 7 degree, 100mm length](https://www.trekbikes.com/p/564745) |
| Size: 60, 62 [Bontrager Pro, 31.8mm, Blendr compatible, 7 degree, 110mm length](https://www.trekbikes.com/p/564746) |
|  | |

[**Weight**](https://www.trekbikes.com/us/en_US/bikes/road-bikes/performance-road-bikes/domane/domane-sl/domane-sl-6/p/28313/?colorCode=black)

|  |  |
| --- | --- |
| Weight | 56 - 9.22 kg / 20.32 lbs |
| Weight limit | This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 275 pounds (125 kg). |