Specifications

*\*spec applies to all sizes unless otherwise noted*

[**Frameset**](https://www.trekbikes.com/au/en_AU/bikes/hybrid-bikes/dual-sport-bikes/dual-sport/dual-sport-3/p/28839/?colorCode=grey)

|  |  |
| --- | --- |
| Frame | Alpha Gold Aluminium, DuoTrap S-compatible, internal cable routing, rack and mudguard mounts, post-mount disc, kickstand mount, 135x5 mm QR |
| Fork | SR Suntour NEX, coil spring, preload, hydraulic lockout, 100x5 mm QR, 63 mm travel |

[**Wheels**](https://www.trekbikes.com/au/en_AU/bikes/hybrid-bikes/dual-sport-bikes/dual-sport/dual-sport-3/p/28839/?colorCode=grey)

|  |  |
| --- | --- |
| Front Hub | Formula DC-20, alloy, 6-bolt, 5x100 mm QR |
| Rear Hub | Formula DC-22, alloy, 6-bolt, Shimano 8/9/10 freehub, 135x5 mm QR |
| Rim | Bontrager Tubeless Ready Disc, 32-hole, Presta valve |
| Spokes | 14 g, stainless |
| Tire | Bontrager GR1 Expert, Hard-Case Lite, wire bead, 60 tpi, 700x40 c |

[**Drivetrain**](https://www.trekbikes.com/au/en_AU/bikes/hybrid-bikes/dual-sport-bikes/dual-sport/dual-sport-3/p/28839/?colorCode=grey)

|  |  |
| --- | --- |
| Shifter | Shimano Acera M3000, 9-speed |
| Front Derailleur | Shimano T3000, 34.9 mm clamp, top swing, dual pull |
| Rear Derailleur | Shimano Acera M3000, Shadow design, long cage |
| \*Crank | Size: S, M Shimano MT210, 46/30, chain guard, 170 mm length |
| Size: L, XL Shimano MT210, 46/30, chain guard, 175 mm length |
| Cassette | Shimano HG200, 11-36, 9-speed |
| Chain | KMC X9, 9-speed |
| Pedal | Wellgo M141, resin body, alloy cage |

[**Components**](https://www.trekbikes.com/au/en_AU/bikes/hybrid-bikes/dual-sport-bikes/dual-sport/dual-sport-3/p/28839/?colorCode=grey)

|  |  |
| --- | --- |
| Saddle | Bontrager H1 |
| Seatpost | Bontrager alloy, 27.2 mm, 12 mm offset, 330 mm length |
| \*Handlebar | Size: S, M Bontrager Comp Lowriser, alloy, 31.8 mm, 15 mm rise, 600 mm width |
| Size: L, XL Bontrager Comp Lowriser, alloy, 31.8 mm, 15 mm rise, 660 mm width |
| Grips | Bontrager XR Endurance Elite, lock-on, ergonomic |
| \*Stem | Size: S Bontrager Elite, 31.8 mm, Blendr-compatible, 7-degree, 80 mm length |
| Size: M, L Bontrager Elite, 31.8 mm, Blendr-compatible, 7-degree, 90 mm length |
| Size: XL Bontrager Elite, 31.8 mm clamp, Blendr-compatible, 7-degree, 110 mm length |
| Headset | 1-1/8" threadless, sealed cartridge bearings |
| \*Brake | Size: S, M, L, XL Shimano MT200 hydraulic disc |
| Size: S, M, L, XL Shimano MT200 hydraulic disc, post-mount, 160 mm rotor |
|  | |

[**Weight**](https://www.trekbikes.com/au/en_AU/bikes/hybrid-bikes/dual-sport-bikes/dual-sport/dual-sport-3/p/28839/?colorCode=grey)

|  |  |
| --- | --- |
| Weight | 13.38 kg / 29.5 lbs |
| Weight limit | This bike has a maximum total weight limit (combined weight of bicycle, rider and cargo) of 136 kg (300 lb). |