Specifications

*\*spec applies to all sizes unless otherwise noted*

[**Frameset**](https://www.trekbikes.com/us/en_US/bikes/hybrid-bikes/fitness-bikes/fx/fx-2-disc/p/27991/?colorCode=black)

|  |  |
| --- | --- |
| Frame | Alpha Gold Aluminum, DuoTrap S compatible, internal cable routing, flat mount disc, rack & fender mounts, 135x5mm QR |
| Fork | FX Alloy, flat mount disc, rack mounts, 405mm axle-to-crown, ThruSkew 5mm QR |

[**Wheels**](https://www.trekbikes.com/us/en_US/bikes/hybrid-bikes/fitness-bikes/fx/fx-2-disc/p/27991/?colorCode=black)

|  |  |
| --- | --- |
| Front Hub | Formula DC-20, alloy, 6-bolt, 5x100mm QR |
| Rear Hub | Formula DC-22, alloy, 6-bolt, Shimano 8/9/10 freehub, 135x5mm QR |
| Rim | Bontrager Connection, alloy, double-wall, 32-hole, schrader valve |
| Spokes | 14g, stainless |
| Tire | Bontrager H2, wire bead, 30 tpi, 700x35c |

[**Drivetrain**](https://www.trekbikes.com/us/en_US/bikes/hybrid-bikes/fitness-bikes/fx/fx-2-disc/p/27991/?colorCode=black)

|  |  |
| --- | --- |
| Shifter | Shimano Altus M310, 8 speed |
| Front Derailleur | Shimano Tourney TY710, 34.9mm clamp, top swing, dual pull |
| Rear Derailleur | Shimano Acera M360, long cage |
| Crank | Forged alloy, 48/38/28, chainguard, 170mm length |
| Cassette | Shimano HG31, 11-32, 8 speed |
| Chain | KMC Z7 |
| Pedal | Bontrager Satellite City pedal |

[**Components**](https://www.trekbikes.com/us/en_US/bikes/hybrid-bikes/fitness-bikes/fx/fx-2-disc/p/27991/?colorCode=black)

|  |  |
| --- | --- |
| Saddle | [Bontrager Sport](https://www.trekbikes.com/p/533016) |
| Seatpost | Bontrager alloy, 27.2mm, 12mm offset, 330mm length |
| \*Handlebar | Size: S, MBontrager alloy, 31.8mm, 15mm rise, 600mm width |
| Size: L, XL, XXLBontrager alloy, 31.8mm, 15mm rise, 660mm width |
| Grips | Bontrager Satellite |
| \*Stem | Size: S, MBontrager alloy, 31.8mm, Blendr compatible, 7 degree, 90mm length |
| Size: L, XL, XXLBontrager alloy, 31.8mm clamp, Blendr compatible, 7 degree, 100mm length |
| Headset | 1-1/8'' threadless, sealed cartridge bearings |
| Brake | Tektro HD-R280 hydraulic disc, flat mount, 160mm rotor |
|  |

[**Weight**](https://www.trekbikes.com/us/en_US/bikes/hybrid-bikes/fitness-bikes/fx/fx-2-disc/p/27991/?colorCode=black)

|  |  |
| --- | --- |
| Weight | L - 11.95 kg / 26.34 lbs |
| Weight limit | This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 300 pounds (136 kg). |