Specifications

* Frameset

**Frame**

700 Series OCLV Carbon, KVF (Kammtail Virtual Foil) tube shape, Adjustable Top Tube IsoSpeed, Micro-adjust seatmast, tapered head tube, BB90, flat mount disc brakes, 12 mm thru-axle, invisible cable routing, control centre, precision water bottle placement, Aero 3S chain keeper, DuoTrap S-compatible

**Fork**

Madone KVF full carbon disc, carbon tapered steerer, carbon dropouts, hidden cable routing, flat-mount disc brake, 12 mm thru-axle

* Wheels

**Wheels**

Bontrager Aeolus XXX 6 Tubeless Ready Disc, 12 mm thru-Axle

**Tyres**

Bontrager R4 320, 320 tpi, 700x25 c

**Max tyre size**

28 c Bontrager tyres (with at least 4 mm of clearance to frame)

* Drivetrain

**Shifters**

Shimano Dura-Ace Di2, 11-speed

**Front derailleur**

Shimano Dura-Ace Di2, braze-on

**Rear derailleur**

Shimano Dura-Ace Di2

**Crank**

Shimano Dura-Ace, 50/34 (compact)

**Bottom bracket**

BB90

**Cassette**

Shimano Dura-Ace, 11-28, 11-speed

**Chain**

Shimano Dura-Ace

**Pedals**

Not included

* Components

**Saddle**

Bontrager Montrose Pro, carbon rails

**Seatpost**

Madone carbon seatpost, 25 mm offset w/integrated light mount

**Handlebar**

Madone-specific adjustable aero VR-CF, internal cable routing

**Grips**

Bontrager tape

**Stem**

Madone-specific internal cable routing

**Head set**

Madone integrated, stainless cartridge bearings, sealed, 1-3/8˝ top, 1.5˝ bottom

**Brake set**

Shimano Dura-Ace flat-mount hydraulic disc

* Weight

**Weight**

56cm – 7.65 kg/16.86 lbs

**Weight limit**

This bike has a maximum total weight limit (combined weight of bicycle, rider and cargo) of 125 kg (275 lb).