Specifications

* Frameset

**Frame**

Alpha Platinum Aluminum, IsoSpeed, tapered head tube, internal derailleur routing, balanced post mount brake, Boost148, G2 Geometry on 29ers

**Fork**

RockShox Judy Gold RL, Solo Air, Motion Control damper, remote lockout, tapered steerer, Boost110, G2 Geometry w/51mm offset on 29ers, 100mm travel (13.5: 80mm travel)

* Wheels

**Front hub**

Bontrager sealed bearing, alloy axle, centerlock, Boost110

**Rear hub**

Bontrager sealed bearing, centerlock, Boost148

**Rims**

Bontrager Kovee 28-hole Tubeless Ready

**Tires**

Bontrager XR2 Team Issue, Tubeless Ready, 120 tpi, aramid bead, 29x2.20˝ (13.5 & 15.5: 27.5x2.20˝)

* Drivetrain

**Shifters**

SRAM NX Eagle, 12 speed

**Rear derailleur**

SRAM NX Eagle, Type 3 Roller Bearing Clutch

**Crank**

SRAM NX Eagle Dub, 30T Direct Mount

**Bottom bracket**

DUB PF92

**Cassette**

SRAM XG-1230 Eagle, 11-50, 12 speed

**Chain**

SRAM NX Eagle

**Pedals**

Not included

* Components

**Saddle**

Bontrager Arvada, hollow chromoly rails

**Seatpost**

Bontrager alloy, 2-bolt head, 31.6mm, 8mm offset

**Handlebar**

Bontrager Comp alloy, 31.8mm, 5mm rise, 720mm width (13.5: 690mm width)

**Grips**

Bontrager XR Trail Comp, nylon lock-on

**Stem**

Bontrager Elite, 31.8mm, 7 degree, Blendr compatible

**Headset**

FSA IS-2, 1-1/8˝ top, 1.5˝ bottom

**Brakeset**

Shimano MT400 hydraulic disc

* Weight

**Weight**

M - 12.20 kg / 26.9 lbs (with tubes)

**Weight limit**

This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 300 pounds (136 kg).