Specifications

*\*spec applies to all sizes unless otherwise noted*

[**Frameset**](https://www.trekbikes.com/us/en_US/bikes/collections/kids-bikes/kids-hybrid-bikes/precaliber/precaliber-16-boys/p/26795/?colorCode=orange)

|  |  |
| --- | --- |
| Frame | Alpha Silver Aluminum, 16'' kids' frame size |
| Fork | Steel, 16'', threadless 1'' steerer |

[**Wheels**](https://www.trekbikes.com/us/en_US/bikes/collections/kids-bikes/kids-hybrid-bikes/precaliber/precaliber-16-boys/p/26795/?colorCode=orange)

|  |  |
| --- | --- |
| Front Hub | Steel, 100mm bolt-on |
| Rear Hub | steel coaster brake hub, 18T sprocket, nutted |
| Rim | Alloy 16'', 28-hole, schrader valve |
| Spokes | 14g stainless steel |
| Tire | Bontrager XR1, wire bead, 27 tpi., 16x2.25'' |

[**Drivetrain**](https://www.trekbikes.com/us/en_US/bikes/collections/kids-bikes/kids-hybrid-bikes/precaliber/precaliber-16-boys/p/26795/?colorCode=orange)

|  |  |
| --- | --- |
| Crank | Alloy, 26T, chainguard, 90mm length |
| Bottom Bracket | Square taper, 68mm, sealed cartridge |
| Chain | HV410, 1/2x1/8 |
| Pedal | Kids' Satellite, 9/16 thread |

[**Components**](https://www.trekbikes.com/us/en_US/bikes/collections/kids-bikes/kids-hybrid-bikes/precaliber/precaliber-16-boys/p/26795/?colorCode=orange)

|  |  |
| --- | --- |
| Saddle | Kids' saddle, small, integrated handle, seat post |
| Handlebar | Steel kid's handlebar, 500mm width, 80mm rise, 25.4mm clamp |
| Grips | Kids' grip, 107mm width |
| Stem | Bontrager Approved, 50mm length, 15 degree rise, 25.4mm clamp |
| Headset | 1'' threadless |

[**Accessories**](https://www.trekbikes.com/us/en_US/bikes/collections/kids-bikes/kids-hybrid-bikes/precaliber/precaliber-16-boys/p/26795/?colorCode=orange)

|  |  |
| --- | --- |
| Training Wheel | Training Wheel Trek Adjustable 12''-16'' |

[**Weight**](https://www.trekbikes.com/us/en_US/bikes/collections/kids-bikes/kids-hybrid-bikes/precaliber/precaliber-16-boys/p/26795/?colorCode=orange)

|  |  |
| --- | --- |
| Weight | 8.16 kg / 17.98 lbs |
| Weight limit | This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 80 pounds (36 kg). |