Specifications

*\*spec applies to all sizes unless otherwise noted*

|  |  |
| --- | --- |
| Frame | 700 Series OCLV Carbon, KVF (Kammtail Virtual Foil) tube shape, adjustable top tube IsoSpeed, invisible cable routing, control center, micro-adjust seat mast, precision water bottle placement, 3S aero chain keeper, DuoTrap S compatible, flat mount disc, 142x12mm thru axle |
| Fork | Madone KVF full carbon, tapered carbon steerer, invisible cable routing, flat mount disc, carbon dropouts, 12x100mm thru axle |

|  |  |
| --- | --- |
| Front Wheel | Bontrager Aeolus Pro 5, OCLV Carbon, Tubeless Ready, 19.5mm rim width, 50mm rim depth, 100x12 thru axle |
| Rear Wheel | Bontrager Aeolus Pro 5, OCLV Carbon, Tubeless Ready, 19.5mm rim width, 50mm rim depth, Shimano 11-speed freehub, 142x12 thru axle |
| Tire | Bontrager R3 Hard-Case Lite, aramid bead, 120 tpi, 700x25c |

|  |  |
| --- | --- |
| Shifter | Shimano Ultegra R8020, 11-speed |
| Front Derailleur | Shimano Ultegra R8000, braze-on |
| Rear Derailleur | Shimano Ultegra R8000, short cage, 30T max cog |
| \*Crank | Size: 50, 52Shimano Ultegra R8000, 50/34 (compact), 170mm length |
| Size: 54, 56Shimano Ultegra R8000, 50/34 (compact), 172.5mm length |
| Size: 58, 60, 62Shimano Ultegra R8000, 50/34 (compact), 175mm length |
| Cassette | Shimano Ultegra R8000, 11-28, 11 speed |
| Chain | Shimano Ultegra HG701, 11-speed |

|  |  |
| --- | --- |
| Saddle | [Bontrager Montrose Elite, titanium rails, 138mm width](https://www.trekbikes.com/p/531344) |
| \*Seatpost | Size: 50, 52, 54, 56Madone aero carbon seatmast cap, integrated light mount, 25mm offset, 160mm length (short) |
| Size: 58, 60, 62Madone aero carbon seatmast cap, integrated light mount, 25mm offset, 205mm length (long) |
| \*Handlebar | Size: 50, 52Trek Madone adjustable aero VR-CF, OCLV Carbon, invisible cable routing, 93mm reach, 123mm drop, 40cm width |
| Size: 54, 56Trek Madone adjustable aero VR-CF, OCLV Carbon, invisible cable routing, 93mm reach, 123mm drop, 42cm width |
| Size: 58, 60, 62Trek Madone adjustable aero VR-CF, OCLV Carbon, invisible cable routing, 93mm reach, 123mm drop, 44cm width |
| Handlebar Tape | [Bontrager Supertack Perf tape](https://www.trekbikes.com/p/503320) |
| \*Stem | Size: 50, 52, 54Trek Madone aero, invisible cable routing, 7 degree, 90mm length |
| Size: 56, 58Trek Madone aero, invisible cable routing, 7 degree, 100mm length |
| Size: 60, 62Trek Madone aero, invisible cable routing, 7 degree, 110mm length |

|  |  |
| --- | --- |
| Weight | 56 - 8.72 kg / 19.23 lbs |
| Weight limit | This bike has a maximum total weight limit (combined weight of bicycle, rider, and cargo) of 275 pounds (125 kg). |